STREET STOCK COMPACTS

Any questions please call

Dave Cline (740)213-3635 or Dan Laughlin (740)-630-7811.

Compact cars will consist of rear-wheel-drive cars 106” factory wheelbase or smaller and any FWD cars EXCEPT for 1985 and older Eldorado, Tornado or Riviera’s.

**Tires and Wheels:**

1. Any air-filled tire PERMITTED. .

2. Factory OEM wheels ONLY.

1. NO studded tires allowed.
2. Wheel weights MUST BE REMOVED.

**Interior/Cage:**

1. Battery may be relocated to inside the car, but NOT mandatory.
2. If it is moved inside, it MUST BE securely bolted to the floor. NO straps, bungee cords or rachet straps.
3. Battery coverings are HIGHLY RECOMMENDED for drivers safety.
4. Fuel tank MAY BE relocated to back seat area or mounted off back seat bar. If mounted to back seat bar, gas tank shelf MUST REMAIN 8 inches off the floor and 8 inches off the package shelf or left in the stock location as long as the fuel tank is in front of the rear axle. NO MORE than 3 gallons of gas in stock tank.
5. Gas tank cover HIGHLY RECOMMENDED.
6. Rear sear bar PERMITTED (4x4x1/4) MAX. A simple 4-point type cage is PERMITTED using 4x4x1/4 MAX.
7. Halo bar is PERMITTED. MUST run vertical for safety purposes only.
8. Front window bar/chain or 9 wire is MANDATORY. Can ONLY attach 6 links on roof and cowl measured from window opening.
9. NO OTHER WELDING PERMITTED ANYWHERE (except where specified).

**Exterior:**

1. All doors, hoods and decklids may be chained, wired or banded in 6 spots ONLY. Sheet metal to sheet metal. You can tuck OR remove the trunk lid. NO CREASING.
2. Headers PERMITTED. NO other aftermarket products than what is listed allowed. Bumpers: 1. ANY tinned style, non-chrome, 1 piece bumper PERMITTED. (Examples: Mazda, Camry, W Body, Caravan, 98-02 Ford style). ABSOLUTELY NO chrome, fabricated, homemade style bumpers allowed! Any questions ask first!!
3. Bumper MAY BE welded directly to the front frame.
4. NO added metal or bumper plate.
5. 3/8 chain MAX may be secured to the bumper and one link ONLY can be welded to the 1st 3 inches of the frame rail.
6. NO SHORTENING of the front frame AT ALL!!!

**Suspension:**

1. MUST BE stock working suspension for the car you are using.
2. NO spring spacers or strut risers.

**Repairs:**

1. (2) 4x4x1/4 fix it plates. Fix it plates CAN BE welded solid. MUST have a 1 inch gap between welds. MUST prove damage. PRE RAN ONLY

If it doesn't say you can do it doesn't mean you can!